Sprint 4

|  |  |
| --- | --- |
| Team ID | PNT2022TMID43478 |
| Project Name | Personal Assistance for Seniors Who Are SelfReliant |

**Code for Simulation:**

#include <WiFi.h>//library for wifi #include <PubSubClient.h>//library for MQtt #include <LiquidCrystal\_I2C.h>

#include "DHT.h"// Library for dht11

#define DHTPIN 15 // what pin we're connected to #define DHTTYPE DHT11 // define type of sensor DHT 11 #define LED 2

DHT dht (DHTPIN, DHTTYPE);// creating the instance by passing pin and typr of dht connected

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "64yf7x"//IBM ORGANITION ID

#define DEVICE\_TYPE "b11m3edevicetype"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "b11m3edeviceid"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "-&EMtr7l-v-Gz2G))e" //Token String data3="";

int buzz= 13;

//-------- Customise the above values --------

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";// Server Name char publishTopic[] = "iot-2/evt/Data/fmt/json";// topic name and type of event perform and format in which data to be send

char subscribetopic[] = "iot-2/cmd/command/fmt/String";// cmd REPRESENT command type AND COMMAND IS TEST OF FORMAT STRING

char authMethod[] = "use-token-auth";// authentication method char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;//client id LiquidCrystal\_I2C lcd(0x27,16,2);

// -

WiFiClient wifiClient; // creating the instance for wificlient

PubSubClient client(server, 1883, callback ,wifiClient); //calling the predefined client id by passing parameter like server id,portand wificredential

void setup()// configureing the ESP32

{

**Serial**.begin(115200); dht.begin(); pinMode(buzz, OUTPUT); pinMode(LED,OUTPUT); delay(10); **Serial**.println(); wificonnect(); mqttconnect();

}

void loop()// Recursive Function

{

if (!client.loop()) { mqttconnect();

}

}

/\*.....................................retrieving to

Cloud. \*/

void PublishData(float temp, float humid) { mqttconnect();//function call for connecting to ibm

}

void mqttconnect() {

if (!client.connected()) { **Serial**.print("Reconnecting client to "); **Serial**.println(server);

while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print("."); delay(500);

}

initManagedDevice();

**Serial**.println();

}

}

void wificonnect() //function defination for wificonnect

{

**Serial**.println(); **Serial**.print("Connecting to ");

WiFi.begin("Wokwi-GUEST", "", 6);//passing the wifi credentials to establish the connection

while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.println(""); **Serial**.println("WiFi connected"); **Serial**.println("IP address: "); **Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

if (client.subscribe(subscribetopic)) { **Serial**.println((subscribetopic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

}

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: ");

**Serial**.println(subscribetopic);

for (int i = 0; i < payloadLength; i++) {

//Serial.print((char)payload[i]); data3 += (char)payload[i];

}

**Serial**.println("Medicine Name: "+ data3); if(data3 != "")

{

lcd.init();

lcd.print(data3); digitalWrite(LED,HIGH); tone(buzz, 100, 1000); delay(2000); digitalWrite(LED,LOW); noTone(buzz); delay(1000);

}

else

{

digitalWrite(LED,LOW);

}

data3="";

}